
! Environment Variables
! ---------------------
ENVIRONMENT 5
  "U" "D:\GPSUSER"
  "T" "D:\TEMPV50"
  "X" "D:\BERN50\GPS"
  "P" "D:\GPSDATA"
  "USER" "bon"
  ## widget = initmenu; pointer = ENVIR_LIST

! Information for the title
! -------------------------
CAMPAIGN 1  "${P}\kinovelap"
  ## widget = initmenu; pointer = ACTIVE_CAMPAIGN

SESSION_TABLE 1  "${P}\kinovelap\STA\SESSIONS.SES"
  ## widget = initmenu; pointer = SESSION_TABLE

DESCR_SESSION_TABLE 1  "Session table"

YR4_INFO 1  "2006"
  ## widget = comment
  # $Y+0

SES_INFO 1  "2160"
  ## widget = comment
  # $S+0

USR_INFO 1  "${USER}"
  ## widget = comment

! -------------------------------------------------------------------------
! Show general files
! ------------------
SHOWGEN 1  "1"
  ## widget = checkbox

MSG_SHOWGEN 1  "Show all general files"

! General Constants
! -----------------
CONST 1  "${X}/GEN\CONST"
  ## widget = selwin; path = PTH_GEN; ext = NO_EXT; maxfiles = 1
  # CONST

DESCR_CONST 1  "General constants"

! Geodetic Datum
! --------------
DATUM 1  "${X}/GEN\DATUM"
  ## widget = selwin; path = PTH_GEN; ext = NO_EXT; maxfiles = 1
  # DATUM

DESCR_DATUM 1  "Geodetic datum"

! Satellite Information
! ---------------------
SATELL 1  "${X}/GEN\SAT_FORSAT3"
  ## widget = selwin; path = PTH_GEN; ext = NO_EXT; maxfiles = 1
  # SAT_FORSAT3

DESCR_SATELL 1  "Satellite information"

! Satellite Problems
! ------------------
SATCRUX 1  "${X}/GEN\SAT_2006.CRX"
  ## widget = selwin; path = PTH_GEN; ext = EXT_CRX; maxfiles = 1
  # SAT_$Y+0

DESCR_SATCRUX 1  "Satellite problems"

! Pole File
! ---------
POLE 1  "${P}\kinovelap\ORB\CODE2160.ERP"
  ## widget = selwin; path = DIR_ERP; ext = EXT_ERP; maxfiles = 1
  # CODE$S+0

DESCR_POLE 1  "Pole file"

! Subdaily Pole Model
! -------------------
SUBMOD 1  "${X}/GEN\IERS2000.SUB"
  ## widget = selwin; path = PTH_GEN; ext = EXT_SUB; maxfiles = 1
  # IERS2000

DESCR_SUBMOD 1  "Subdaily pole model"

! Nutation Model
! -------------------
NUTMOD 1  "${X}/GEN\IAU2000.NUT"
  ## widget = selwin; path = PTH_GEN; ext = EXT_NUT; maxfiles = 1
  # IAU2000

DESCR_NUTMOD 1  "Nutation model"

! Phase Center Eccentricities
! ---------------------------
PHASECC 1  "${X}/GEN\PHAS_IGS.REL"
  ## widget = selwin; path = PTH_GEN; ext = NO_EXT; maxfiles = 1
  # PHAS_IGS.REL

DESCR_PHASECC 1  "Phase center eccentricities"

! Zero-Difference Header File(s)
! --------------------------------
RADIO_Z 1  "1"
  ## widget = radiobutton; group = OBSFILES; radiokeys = PZFILES

MSG_RADIO_Z 1  "Zero-difference observation files"

PZFILES 1  "${P}\kinovelap\OBS\POD12160.PZH"
  ## widget = selwin; path = DIR_PZH; ext = EXT_PZH; maxfiles = 999
  ## emptyallowed = true
  # ????$S+0

PZFILES_TXT_COL_1 1  "Zero-difference header file"

MSG_PZFILES 1  "Zero-difference observation files"

! Extensions of the Zero-Difference Obs. Files
! ----------------------------------------------
PZFILES_PTH_COL_2 1  "${P}\kinovelap\OBS\"
  ## widget = initmenu; pointer = DIR_PZO

PZFILES_EXT_COL_2 1  "PZO"
  ## widget = initmenu; pointer = EXT_PZO

PZFILES_TXT_COL_2 1  "Zero-difference obs file"

! Single-Difference Header File(s)
! --------------------------------
RADIO_S 1  "0"
  ## widget = radiobutton; group = OBSFILES; radiokeys = OBSFIL

MSG_RADIO_S 1  "Single-difference observation files"

OBSFIL 0
  ## widget = selwin; path = DIR_PSH; ext = EXT_PSH; maxfiles = 999
  ## emptyallowed = true
  # 

OBSFIL_TXT_COL_1 1  "Single-difference header file"

MSG_OBSFIL 1  "Single-difference observation files"

! Extensions of the Single-Difference Obs. Files
! ----------------------------------------------
OBSFIL_PTH_COL_2 1  "${P}\kinovelap\OBS\"
  ## widget = initmenu; pointer = DIR_PSO

OBSFIL_EXT_COL_2 1  "PSO"
  ## widget = initmenu; pointer = EXT_PSO

OBSFIL_TXT_COL_2 1  "Single-difference obs file"

! A Priori Coordinates
! --------------------
COORD 1  "${P}\kinovelap\STA\IGS_00.CRD"
  ## widget = selwin; path = DIR_CRD; ext = EXT_CRD; maxfiles = 1
  # IGS_00

DESCR_COORD 1  "A priori coordinates"

! GNSS Standard Orbits
! --------------------
STDORB 1  "${P}\kinovelap\ORB\GPS.STD"
  ## widget = selwin; path = DIR_STD; ext = EXT_STD; maxfiles = 1
  # GPS

DESCR_STDORB 1  "GNSS standard orbits"

! Atmosphere: Meteo File
! ----------------------
METFIL 0
  ## widget = selwin; path = DIR_MET; ext = EXT_MET; maxfiles = 999
  ## emptyallowed = true
  # 

MSG_METFIL 1  "Meteo data files"

! Atmosphere: Tropospheric Model
! ------------------------------
TROPOS 1  "NONE"
  ## widget = combobox; editable = false
  ## cards = SAASTAMOINEN HOPFIELD ESSEN-FROOME NIELL DRY_SAAST DRY_HOPFIELD DRY_NIELL NONE

MSG_TROPOS 1  "ZPD model and mapping function"

! Atmosphere: Troposphere Estimates
! ---------------------------------
TROPEST 0
  ## widget = selwin; path = DIR_TRP; ext = EXT_TRP; maxfiles = 1
  ## emptyallowed = true
  # 

DESCR_TROPEST 1  "Estimated troposphere values"

! Ionosperic Model
! ----------------
IONOS 0
  ## widget = selwin; path = DIR_ION; ext = EXT_ION; maxfiles = 1
  ## emptyallowed = true
  # 

DESCR_IONOS 1  "Ionosphere models"

! Eccentricities
! --------------
ECCENT 0
  ## widget = selwin; path = DIR_ECC; ext = EXT_ECC; maxfiles = 1
  ## emptyallowed = true
  # 

DESCR_ECCENT 1  "Site eccentricities"

! Kinematic positions, input
! --------------------------
KININP 0
  ## widget = selwin; path = DIR_KIN; ext = EXT_KIN; maxfiles = 1
  ## emptyallowed = true
  # 

DESCR_KININP 1  "Kinematic input coordinates"

! Satellite Clocks
! ----------------
SATCLK 1  "${P}\kinovelap\ORB\CODE2160.CLK"
  ## widget = selwin; path = DIR_CLK; ext = EXT_CLK; maxfiles = 1
  ## emptyallowed = true
  # CODE$S+0

DESCR_SATCLK 1  "Satellite clocks"

! LEO Kinematic positions
! -----------------------
LEOPROC 1  "1"
  ## widget = checkbox

MSG_LEOPROC 1  "Process LEOs"

! LEO Standard Orbits
! -------------------
LEOSTD 1  "${P}\kinovelap\ORB\0424ph2.STD"
  ## widget = selwin; path = DIR_STD; ext = EXT_STD; maxfiles = 1
  ## emptyallowed = true
  # 0424ph2

DESCR_LEOSTD 1  "LEO standard orbit"

! LEO Kinematic velocities
! ------------------------
KINVEL 0
  ## widget = selwin; path = DIR_KVL; ext = EXT_KVL; maxfiles = 1
  ## emptyallowed = true
  # 

DESCR_KINVEL 1  "Kinematic velocities"

! LEO attitude
! ------------
ATTIT 1  "${P}\kinovelap\ORB\POD12160.ATT"
  ## widget = selwin; path = DIR_ATT; ext = EXT_ATT; maxfiles = 1
  ## emptyallowed = true
  # ????$S+0

DESCR_ATTIT 1  "LEO attitude"

! GPS-UTC file
! -------------
GPSUTC 1  "${X}/GEN\GPSUTC"
  ## widget = selwin; path = PTH_GEN; ext = NO_EXT; maxfiles = 1
  # GPSUTC

DESCR_GPSUTC 1  "Difference GPS-UTC"

! STAINFO file
! ------------
STAINFO 1  "${P}\kinovelap\STA\ITRFCODE.STA"
  ## widget = selwin; path = DIR_STA; ext = EXT_STA; maxfiles = 1
  ## emptyallowed = true
  # ITRFCODE

DESCR_STAINFO 1  "Station information"

! Resulting Coordinates
! ---------------------
COORDRS 0
  ## widget = lineedit; path = DIR_CRD; ext = EXT_CRD
  # 

DESCR_COORDRS 1  "Coordinate results"

! Residuals
! ---------
RESIDRS 1  "${P}\kinovelap\OUT\MAUPRP.RES"
  ## widget = lineedit; path = DIR_RES; ext = EXT_RES
  # MAUPRP

DESCR_RESIDRS 1  "Residual file"

! Scratch Files
! -------------
AUXFIL 1  "${U}/WORK\MAUPRP.SCR"
  ## widget = lineedit; path = PTH_SCR; ext = EXT_SCR; emptyallowed = false
  # MAUPRP$J

DESCR_AUXFIL 1  "Scratch file"

OBCOPY 1  "${U}/WORK\MAUPRP.SC1"
  ## widget = lineedit; path = PTH_SCR; ext = EXT_SC1; emptyallowed = false
  # MAUPRP$J

DESCR_OBCOPY 1  "Scratch file"

DELETE_FILES 2
  "AUXFIL"
  "OBCOPY"

! Program Output File
! -------------------
SYSODEF 1  "1"
  ## widget = checkbox

MSG_SYSODEF 1  "Program output"

SYSOUT 1  "${P}\kinovelap\OUT\MAUPRP.L03"
  ## widget = lineedit; path = DIR_OUT; ext = EXT_OUT
  ## activeif = SYSODEF == 0; emptyallowed = false
  # MAUPRP

DESCR_SYSOUT 1  "Program output"

! Error Message File
! ------------------
ERRMRG 1  "0"
  ## widget = checkbox

MSG_ERRMRG 1  "Error message"

SYSERR 1  "${U}/WORK\ERROR.MSG"
  ## widget = lineedit; path = PTH_ERR; ext = EXT_ERR
  ## activeif = ERRMRG == 0; emptyallowed = false
  # ERROR

DESCR_SYSERR 1  "Error message"

! Program title
! -------------
TITLE 1  "cycle slip detection"
  ## widget = lineedit

MSG_TITLE 1  "Title line"

! Processing IAUTO
! ---------------
! IAUTO 1  "AUTOMATIC"
!   ## widget = combobox; editable = false; cards = AUTOMATIC MANUAL
IAUTO 1  "AUTOMATIC"
  ## widget = combobox; editable = false; cards = AUTOMATIC

! Adjust Frequencies/Wave-length Factors
! --------------------------------------
ISETOP 1  "1"
  ## widget = checkbox

MSG_ISETOP 1  "Adjust freq./wlfac."

! Frequencies
! -----------
NFRCHK 1  "COMBINED"
  ## widget = combobox; editable = false; cards = COMBINED BOTH L1 L2

MSG_NFRCHK 1  "Screening mode, frequency to check"

! Save Screened Files
! -------------------
ISAVE 1  "1"
  ## widget = checkbox

MSG_ISAVE 1  "Save screened observation files"

! Use marking flags
! -----------------
IUSFLG 1  "0"
  ## widget = checkbox

MSG_IUSFLG 1  "Mark if marking flags in observation file"

! Mark Unpaired Observations
! --------------------------
MRK1O2 1  "1"
  ## widget = checkbox

MSG_MRK1O2 1  "Mark unpaired dual frequency observations"

! Minimal Elevation
! -----------------
MINEL 1  "3"
  ## widget = spinbox; range = -90 90 1

MSG_MINEL 1  "Mark observations below an elevation of for stations"

! Minimal Elevation for LEO
! -------------------------
MINELEO 1  "0"
  ## widget = spinbox; range =-45 90 1; activeif = LEOPROC = 1

MSG_MINELEO 1  "Mark observations below an elevation of for LEOs"

! Minimal Time for Contineous Obs.
! --------------------------------
MNCONT 1  "151"
  ## widget = lineedit

MSG_MNCONT 1  "Minimum time interval accepted for continuous observations"

! Maximal Gap in Observartions
! ----------------------------
MXHOLE 1  "61"
  ## widget = lineedit

MSG_MXHOLE 1  "Maximum gap accepted within continuous observations"

! Printing flag
! -------------
IPRNT1 1  "SUMMARY"
  ## widget = combobox; editable = false; cards = SUMMARY DETAILS NONE

MSG_IPRNT1 1  "Extent of program output"

! Single-Difference Screening
! ---------------------------
IPPROC1 1  "0"
  ## widget = checkbox

MSG_IPPROC1 1  "Original observations from file"

! Double-Difference Screening
! ---------------------------
IPPROC2 1  "1"
  ## widget = checkbox

MSG_IPPROC2 1  "Differences between satellites"

! Maximal Interval of Fit
! -----------------------
MXINTR 1  "2"
  ## widget = lineedit

MSG_MXINTR 1  "Maximum time interval for polynomial fit"

! Frequency used for Triple-Dif. Solution
! ---------------------------------------
LTRIP 1  "L3"
  ## widget = combobox; editable = false; cards = L3 L1 L2 L5

MSG_LTRIP 1  "Frequency for the solution"

! Kinematic or Static Coordinate Estimation
! ------------------------------------------
KINSTA 1  "1"
  ## widget = checkbox

MSG_KINSTA 1  "Kinematic coordinate estimation"

! A Priori Weights
! ----------------
APRCWGT 1  "1"
  ## widget = checkbox

MSG_APRCWGT 1  "A priori coordinate/baseline vector sigmas"

! Maximum Observed-Computed Value
! -------------------------------
OMCMAX 1  "0.5"
  ## widget = lineedit

MSG_OMCMAX 1  "Maximum observed-computed value"

! RMS limit for epoch solution
! ----------------------------
RMSMAX 1  "0.042"
  ## widget = lineedit; activeif = KINSTA = 1 OR RADIO_Z = 1
  ## check_type = real; check_min = 0.0

MSG_RMSMAX 1  "RMS limit for epoch solution"

! Polynomial Degree (Single-Dif.)
! -------------------------------
QQ1 1  "1"
  ## widget = spinbox; range = 1 4 1; activeif = IPPROC1 = 1

MSG_QQ1 1  "Polynomial degree"

! Discontinuity Level (Single-Dif.)
! ---------------------------------
DISCLV1 1  "0.4"
  ## widget = lineedit; activeif = IPPROC1 = 1; check_type = real
  ## check_min = 0.0

MSG_DISCLV1 1  "Discontinuity level"

! Polynomial Degree (Double-Dif.)
! -------------------------------
QQ2 1  "1"
  ## widget = spinbox; range = 1 4 1; activeif = IPPROC2 = 1

MSG_QQ2 1  "Polynomial degree"

! Discontinuity Level (Double-Dif.)
! ---------------------------------
DISCLV2 1  "0.1"
  ## widget = lineedit; activeif = IPPROC2 = 1; check_type = real
  ## check_min = 0.0

MSG_DISCLV2 1  "Discontinuity level"

! Apriori Weight (X-Coordinate)
! -----------------------------
SIGWGS1 1  "0.01"
  ## widget = lineedit; activeif = APRCWGT = 1; check_type = real
  ## check_min = 0.0

MSG_SIGWGS1 1  "X-coordinate"

! Apriori Weight (Y-Coordinate)
! -----------------------------
SIGWGS2 1  "0.01"
  ## widget = lineedit; activeif = APRCWGT = 1; check_type = real
  ## check_min = 0.0

MSG_SIGWGS2 1  "Y-coordinate"

! Apriori Weight (Z-Coordinate)
! -----------------------------
SIGWGS3 1  "0.01"
  ## widget = lineedit; activeif = APRCWGT = 1; check_type = real
  ## check_min = 0.0

MSG_SIGWGS3 1  "Z-coordinate"

! Minimum size if a clock event
! -----------------------------
CLKOPT2 1  "50"
  ## widget = lineedit; check_type = integer; check_min = 1

MSG_CLKOPT2 1  "Minimum size of a clock event"

! Tolerance for MS jump detection
! -------------------------------
TOLJMP 1  "0.001"
  ## widget = lineedit; check_type = real; check_min = 0

MSG_TOLJMP 1  "Tolerance for ms-jump detection"

! Deletion flag for file with ms-jumps
! ------------------------------------
CLKOPT5 1  "0"
  ## widget = checkbox

MSG_CLKOPT5 1  "Flag the observation file for deletion"

! Repair the ms-jumps
! -------------------
CLKOPT1 1  "1"
  ## widget = checkbox; activeif = CLKOPT5 = 0

MSG_CLKOPT1 1  "Repair the ms-jumps as cycle slips"

! Deletion flag for file with clock events
! ----------------------------------------
CLKOPT6 1  "0"
  ## widget = checkbox

MSG_CLKOPT6 1  "Flag the observation file for deletion"

! Mark observations up to a time interval
! ---------------------------------------
CLKOPT3 1  "300"
  ## widget = lineedit; emptyallowed = true; activeif = CLKOPT6 = 0
  ## check_type = integer; check_min = 1

MSG_CLKOPT3 1  "Mark observations up to a time interval"

! Ambiguities for all satellites
! ------------------------------
CLKOPT4 1  "1"
  ## widget = checkbox; activeif = CLKOPT6 = 0

MSG_CLKOPT4 1  "Set ambiguities for all satellites"

! Fixed Station
! -------------
STAFIX 0
  ## widget = selwin; maxfiles = 1; pointer = STALST
  ## activeif = RADIO_S = 1 AND COORDRS / _
  # 

MSG_STAFIX 1  "Define the fixed station"

STALST 0
  ## widget = selwin; menuaux = MENUAUX; action = OBS
  ## menuauxkeys = CONST OBSFIL

! Print Cycle-Slip Detection Flag
! -------------------------------
IPRNT2 1  "SUMMARY"
  ## widget = combobox; editable = false; cards = SUMMARY DETAILS NONE

MSG_IPRNT2 1  "Extent of program output"

! Sigma of L1 Observation
! -----------------------
SIGL12_1 1  "0.0010"
  ## widget = lineedit; activeif = NFRCHK == COMBINED

MSG_SIGL12_1 1  "Sigma for L1 observations"

! Sigma of L2 Observation
! -----------------------
SIGL12_2 1  "0.0010"
  ## widget = lineedit; activeif = NFRCHK == COMBINED

MSG_SIGL12_2 1  "Sigma for L2 observations"

! Full or Half Cycles L1
! ----------------------
IWLSCR1 1  "FULL"
  ## widget = combobox; editable = false; cards = FULL HALF
  ## activeif = ISETOP == 0

MSG_IWLSCR1 1  "Search L1 for"

! Full or Half Cycles L2
! ----------------------
IWLSCR2 1  "FULL"
  ## widget = combobox; editable = false; cards = FULL HALF
  ## activeif = ISETOP == 0

MSG_IWLSCR2 1  "Search L2 for"

! Test only Flagged Observations
! ------------------------------
NTONLY 1  "0"
  ## widget = checkbox

MSG_NTONLY 1  "Test only observations with cycle slip flag"

! L5 is Clean
! -----------
L5CLEA 1  "0"
  ## widget = checkbox

MSG_L5CLEA 1  "L5 is clean except for observations with flags"

! Search Width L1
! ---------------
SWIDTH1 1  "5"
  ## widget = spinbox; range = 3 6 1; activeif = NFRCHK = COMBINED

MSG_SWIDTH1 1  "Search width to find L1 cycle slip correction"

! Search Width L5
! ---------------
SWIDTH2 1  "2"
  ## widget = spinbox; range = 1 3 1; activeif = NFRCHK = COMBINED

MSG_SWIDTH2 1  "Search width to find L5 cycle slip correction"

! Enable Solution of Cycle Slips
! ------------------------------
CYCDET 1  "1"
  ## widget = checkbox

MSG_CYCDET 1  "Do not accept cycle slip corrections"

! Minimal Size of Cycle-Slip
! --------------------------
MINCYC 1  "10"
  ## widget = lineedit; check_type = integer; check_min = 0
  ## activeif = CYCDET = 0

MSG_MINCYC 1  "Minimum size of accepted cycle slip correction"

! Outlier Rejection
! -----------------
IRJECT 1  "1"
  ## widget = checkbox

MSG_IRJECT 1  "Enable outlier rejection"

! Maximal Observation Gap
! -----------------------
MXOGAP 1  "91"
  ## widget = lineedit

MSG_MXOGAP 1  "Mark consecutive outliers up to a time interval"

! Maximal Ionosphere Difference
! -----------------------------
MXIOND 1  "999"
  ## widget = lineedit

MSG_MXIOND 1  "Maximum ionospheric change from epoch to epoch"

! Set a New Ambiguity Flags
! -------------------------
IAMNEW1 1  "0"
  ## widget = checkbox

MSG_IAMNEW1 1  "If a cycle slip flag in observation file"

IAMNEW2 1  "1"
  ## widget = checkbox

MSG_IAMNEW2 1  "If no cycle slip correction was possible"

IAMNEW3 1  "91"
  ## widget = lineedit

MSG_IAMNEW3 1  "After an observation gap larger than"

IAMNEW4 1  "0"
  ## widget = checkbox

MSG_IAMNEW4 1  "Preserve ambiguities from observation file"

IAMNEW5 1  "151"
  ## widget = lineedit

MSG_IAMNEW5 1  "Minimum observed time interval per ambiguity"

! Maximum number of ambiguities
! -----------------------------
MXAMBS 1  "999"
  ## widget = lineedit

MSG_MXAMBS 1  "Remove satellites if the file contains more than"


# BEGIN_PANEL NO_CONDITION #####################################################
# PREPROCESSING OF ZERO-/SINGLE-DIFF. PHASE OBS. FILES - MAUPRP 1: Input Files #
#                                                                              #
# GENERAL FILES                                                                #
#   Show all general files                    > % <                            # SHOWGEN
#                                                                              #
# INPUT FILES                                                                  #
# > % <Zero-difference observation files      > %%%%%%%% <                     # RADIO_Z PZFILES
# > % <Single-difference observation files    > %%%%%%%% <                     # RADIO_S OBSFIL
#   A priori coordinates                      > %%%%%%%% <                     # COORD
#   Site eccentricities                       > %%%%%%%% <                     # ECCENT
#   Kinematic input coordinates               > %%%%%%%% <                     # KININP
#   GNSS standard orbits                      > %%%%%%%% <                     # STDORB
#   Pole file                                 > %%%%%%%% <                     # POLE
#   Satellite clocks                          > %%%%%%%% <                     # SATCLK
#   Estimated troposphere values              > %%%%%%%% <                     # TROPEST
#   Meteo data files                          > %%%%%%%% <                     # METFIL
#   Ionosphere models                         > %%%%%%%% <                     # IONOS
#   Process LEOs                              > % <                            # LEOPROC
# END_PANEL ####################################################################


# BEGIN_PANEL SHOWGEN = 1 ######################################################
# MAUPRP 1.1: General Files                                                    #
#                                                                              #
# GENERAL INPUT FILES                                                          #
#   General constants           > %%%%%%%%%%%% <                               # CONST
#   Geodetic datum              > %%%%%%%%%%%% <                               # DATUM
#   Subdaily pole model         > %%%%%%%%%%%% <                               # SUBMOD
#   Nutation model              > %%%%%%%%%%%% <                               # NUTMOD
#   Satellite information       > %%%%%%%%%%%% <                               # SATELL
#   Satellite problems          > %%%%%%%%%%%% <                               # SATCRUX
#   Station information         > %%%%%%%%%%%% <                               # STAINFO
#   Phase center eccentricities > %%%%%%%%%%%% <                               # PHASECC
#                                                                              #
# MENU SETTINGS                                                                #
#   Selected campaign           > %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%% <# CAMPAIGN
#   Selected session              year> %%%% <  session> %%%% <                # YR4_INFO SES_INFO
#   Session table               > %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%% <# SESSION_TABLE
#                                                                              #
# TEMPORARY FILES                                                              #
#   Scratch files               > %%%%%%%%%%%% <          > %%%%%%%%%%%% <     # AUXFIL OBCOPY
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL LEOPROC = 1 ######################################################
# MAUPRP 1.2: LEO Processing                                                   #
#                                                                              #
# INPUT FILES FOR LEO PROCESSING                                               #
#   LEO standard orbit    > %%%%%%%% <                                         # LEOSTD
#   LEO attitude          > %%%%%%%% <                                         # ATTIT
#   GPS-UTC seconds       > %%%%%%%%%%%% <     (only with JASON attitude file) # GPSUTC
#                                                                              #
#   Kinematic velocities  > %%%%%%%% <                                         # KINVEL
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# MAUPRP 2: Output Files                                                       #
#                                                                              #
# RESULT FILES                                                                 #
#   Coordinate results      > %%%%%%%% <                                       # COORDRS
#   Residual file           > %%%%%%%% <                                       # RESIDRS
#                                                                              #
# GENERAL OUTPUT FILES                                                         #
#   Program output          > % < use MAUPRP.Lnn            or    > %%%%%%%% < # SYSODEF SYSOUT
#   Error messages          > % < merged to program output  or    > %%%%%%%% < # ERRMRG SYSERR
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# MAUPRP 3: General Options                                                    #
#                                                                              #
# TITLE  > %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%% <  # TITLE
#                                                                              #
# GENERAL SETTINGS                                                             #
#   Screening mode, frequency to check          > %%%%%%%%% <                  # NFRCHK
#   Save screened observation files             > % <                          # ISAVE
#                                                                              #
# TROPOSPHERE MODELING                                                         #
#   ZPD model and mapping function              > %%%%%%%%%%%%% <              # TROPOS
#                                                                              #
# SAVING COORDINATES                                                           #
#   Define the fixed station                    > %%%%%%%%%%%%%%%% <           # STAFIX
#                                                 (blank: automatic selection) #
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# MAUPRP 4: Marking of Observations                                            #
#                                                                              #
# MARKING OF OBSERVATIONS BEFORE CYCLE SLIP DETECTION                          #
#   Mark if marking flags in observation file                  > % <           # IUSFLG
#   Mark observations below an elevation of     for stations   > %%% <  degrees# MINEL
#                                               for LEOs       > %%% <  degrees# MINELEO
#   Mark unpaired dual frequency observations                  > % <           # MRK1O2
#   Minimum time interval accepted for continuous observations > %%%% < seconds# MNCONT
#   Maximum gap accepted within continuous observations        > %%%% < seconds# MXHOLE
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# MAUPRP 5: Non-Parametric Screening                                           #
#                                                                              #
# GENERAL OPTIONS                                                              #
#   Extent of program output                      > %%%%%%%% <                 # IPRNT1
#   Maximum time interval for polynomial fit      > %% < minutes               # MXINTR
#                                                                              #
# SCREENING ON DIFFERENT DIFFERENCE LEVELS                                     #
#   > % < Original observations from file       for ZD-files: zero   diff.     # IPPROC1
#            Polynomial degree    > % <             SD-files: single diff.     # QQ1
#            Discontinuity level  > %%%%% < meters                             # DISCLV1
#                                                                              #
#   > % < Differences between satellites        for ZD-files: single diff.     # IPPROC2
#            Polynomial degree    > % <             SD-files: double diff.     # QQ2
#            Discontinuity level  > %%%%% < meters                             # DISCLV2
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# MAUPRP 6: Epoch-Difference Solution                                          #
#                                                                              #
# EPOCH-DIFFERENCE SOLUTION                     for ZD-files: double diff.     #
#   Frequency for the solution       > %%% <        SD-files: triple diff.     # LTRIP
#   Kinematic coordinate estimation  > % <                                     # KINSTA
#   Maximum observed-computed value  > %%%%% <  meters   (0.0: no check)       # OMCMAX
#   RMS limit for epoch solution     > %%%%% <  meters   (0.0: no check)       # RMSMAX
#                                                                              #
#  > % < A priori coordinate/baseline vector sigmas                            # APRCWGT
#        X-coordinate                > %%%%%% < meters                         # SIGWGS1
#        Y-coordinate                > %%%%%% < meters                         # SIGWGS2
#        Z-coordinate                > %%%%%% < meters                         # SIGWGS3
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL RADIO_Z = 1 ######################################################
# MAUPRP 7: Clock Events                                                       #
#                                                                              #
# DETECTION OF CLOCK EVENTS                                                    #
#   Minimum size of a clock event          > %%%%%% < nanoseconds              # CLKOPT2
#   Tolerance for ms-jump detection        > %%%%%% < milliseconds             # TOLJMP
#                                                                              #
# MS-JUMP HANDLING                                                             #
#   Flag the observation file for deletion > % <                               # CLKOPT5
#   Repair the ms-jumps as 'cycle slips'   > % <                               # CLKOPT1
#                                                                              #
# HANDLING OF OTHER CLOCK EVENTS                                               #
#   Flag the observation file for deletion > % <                               # CLKOPT6
#   Mark observations up to a time interval> %%%%%% < seconds (blank: no mark) # CLKOPT3
#   Set ambiguities for all satellites     > % <                               # CLKOPT4
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# MAUPRP 8: Cycle Slip Detection/Correction                                    #
#                                                                              #
# CYCLE SLIP DETECTION                                                         #
#   Extent of program output                       > %%%%%%%% <                # IPRNT2
#   Do not accept cycle slip corrections           > % <                       # CYCDET
#   Minimum size of accepted cycle slip correction > %%%%%%%% < cycles         # MINCYC
#   Test only observations with cycle slip flag    > % <                       # NTONLY
#   L5 is clean except for observations with flags > % <                       # L5CLEA
#                                                                              #
# NO CYCLE SLIP HYPOTHESIS                                                     #
#   Sigma for L1 observations                      > %%%%%% <  meters          # SIGL12_1
#   Sigma for L2 observations                      > %%%%%% <  meters          # SIGL12_2
#   Maximum ionospheric change from epoch to epoch > %%%%%% <  % of L1 cycles  # MXIOND
#                                                                              #
# CYCLE SLIP CORRECTIONS                                                       #
#   Search width to find L1 cycle slip correction  > % <       integers        # SWIDTH1
#   Search width to find L5 cycle slip correction  > % <       integers        # SWIDTH2
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# MAUPRP 9: Outlier Rejection / Ambiguity Setting                              #
#                                                                              #
# OUTLIER REJECTION                                                            #
#   Enable outlier rejection                            > % <                  # IRJECT
#   Mark consecutive outliers up to a time interval     > %%%% <  seconds      # MXOGAP
#                                                                              #
# SET UP MULTIPLE AMBIGUITIES                                                  #
#   Preserve ambiguities from observation file          > % <                  # IAMNEW4
#   If a cycle slip flag in observation file            > % <                  # IAMNEW1
#   If no cycle slip correction was possible            > % <                  # IAMNEW2
#   After an observation gap larger than                > %%%% <  seconds      # IAMNEW3
#                                                                              #
# MARKING OF OBSERVATIONS AFTER CYCLE SLIP CORRECTIONS                         #
#   Minimum observed time interval per ambiguity        > %%%% <  seconds      # IAMNEW5
#   Remove satellites if the file contains more than    > %%%% <  ambiguities  # MXAMBS
#                                                                              #
# END_PANEL ####################################################################
