
! Environment Variables
! ---------------------
ENVIRONMENT 7
  "U" "/u/aiub/bern50/GPSUSER"
  "T" "/scratch/bern50"
  "X" "/aiub_sw/BERN50/GPS"
  "P" "/aiub"
  "Q" "/aiub2"
  "K" "/aiub_u_camp"
  "USER" "bern50"
  ## widget = initmenu; pointer = ENVIR_LIST

! SOME KEYWORDS FOR AUTOMATIC OUTPUT
! ----------------------------------
CAMPAIGN 1  "${Q}/EXAMPLE"
  ## widget = initmenu; pointer = ACTIVE_CAMPAIGN

SESSION_TABLE 1  "${Q}/EXAMPLE/STA/SESSIONS.SES"
  ## widget = initmenu; pointer = SESSION_TABLE

DESCR_SESSION_TABLE 1  "Session table"

YR4_INFO 1  "2002"
  ## widget = comment
  # $Y+0

SES_INFO 1  "1430"
  ## widget = comment
  # $S+0

USR_INFO 1  "${USER}"
  ## widget = comment

! -------------------------------------------------------------------------
! Show general files
! ------------------
SHOWGEN 1  "1"
  ## widget = checkbox

MSG_SHOWGEN 1  "Show all general files"

! General Constants
! -----------------
CONST 1  "${X}/GEN/CONST."
  ## widget = selwin; path = PTH_GEN; ext = NO_EXT; maxfiles = 1
  # CONST.

DESCR_CONST 1  "General constants"

! Local Geodetic Datum
! --------------------
DATUM 1  "${X}/GEN/DATUM."
  ## widget = selwin; path = PTH_GEN; ext = NO_EXT; maxfiles = 1
  # DATUM.

DESCR_DATUM 1  "Geodetic datum"

! Satellite Information
! ---------------------
SATELL 1  "${X}/GEN/SATELLIT."
  ## widget = selwin; path = PTH_GEN; ext = NO_EXT; maxfiles = 1
  # SATELLIT.

DESCR_SATELL 1  "Satellite information"

! Satellite Problems
! ------------------
SATCRUX 1  "${X}/GEN/SAT_2002.CRX"
  ## widget = selwin; path = PTH_GEN; ext = EXT_CRX; maxfiles = 1
  # SAT_$Y+0

DESCR_SATCRUX 1  "Satellite problems"

! Station crux file
! -----------------
STAINFO 0
  ## widget = selwin; path = DIR_STA; ext = EXT_STA; maxfiles = 1
  ## emptyallowed = true
  # 

DESCR_STAINFO 1  "Station information"

! Receiver information
! --------------------
RECEIVR 1  "${X}/GEN/RECEIVER."
  ## widget = selwin; path = PTH_GEN; ext = NO_EXT; maxfiles = 1
  ## emptyallowed = true
  # RECEIVER.

DESCR_RECEIVR 1  "Receiver information"

! Pole File
! ---------
POLE 1  "${Q}/EXAMPLE/ORB/IGS021430.ERP"
  ## widget = selwin; path = DIR_ERP; ext = EXT_ERP; maxfiles = 1
  # $B$YSS+0

DESCR_POLE 1  "Pole file"

! Subdaily Pole Model
! -------------------
SUBMOD 1  "${X}/GEN/IERS2000.SUB"
  ## widget = selwin; path = PTH_GEN; ext = EXT_SUB; maxfiles = 1
  # IERS2000

DESCR_SUBMOD 1  "Subdaily pole model"

! Nutation Model
! -------------------
NUTMOD 1  "${X}/GEN/IAU2000.NUT"
  ## widget = selwin; path = PTH_GEN; ext = EXT_NUT; maxfiles = 1
  # IAU2000

DESCR_NUTMOD 1  "Nutation model"

! Phase Center Eccentricities
! ---------------------------
PHASECC 1  "${X}/GEN/PHAS_IGS.REL"
  ## widget = selwin; path = PTH_GEN; ext = EXT_ANY; maxfiles = 1
  # PHAS_IGS.REL

DESCR_PHASECC 1  "Phase center eccentricities"

! Broadcast Ephemeris
! -------------------
RADIO_B 1  "0"
  ## widget = radiobutton; group = ORBIT; radiokeys = BRDEPH

MSG_RADIO_B 1  "Broadcast orbits"

BRDEPH 0
  ## widget = selwin; path = DIR_BRD; ext = EXT_BRD; maxfiles = 1
  ## emptyallowed = true
  # 

DESCR_BRDEPH 1  "Broadcast orbits"

! Standard Orbits
! ---------------
RADIO_S 1  "1"
  ## widget = radiobutton; group = ORBIT; radiokeys = STDORB SATCLK

MSG_RADIO_S 1  "Selection of standard orbit"

STDORB 1  "${Q}/EXAMPLE/ORB/IGS021430.STD"
  ## widget = selwin; path = DIR_STD; ext = EXT_STD; maxfiles = 1
  ## emptyallowed = true
  # $B$YSS+0

DESCR_STDORB 1  "Standard orbits"

! Satellite Clocks
! ----------------
SATCLK 1  "${Q}/EXAMPLE/ORB/$G021430.CLK"
  ## widget = selwin; path = DIR_CLK; ext = EXT_CLK; maxfiles = 1
  ## emptyallowed = true
  # $G$YSS+0

DESCR_SATCLK 1  "Satellite clocks"

! Code Files
! ----------
CODEFILE 1  "${Q}/EXAMPLE/OBS/$(FFFF)1430.CZH"
  ## widget = selwin; path = DIR_CZH; ext = EXT_CZH; maxfiles = 999
  # SELECTED

MSG_CODEFILE 1  "Code observation files"

! File Extensions
! ---------------
CODEFILE_PTH_COL_2 1  "${Q}/EXAMPLE/OBS/"
  ## widget = initmenu; pointer = DIR_CZO

CODEFILE_EXT_COL_2 1  "CZO"
  ## widget = initmenu; pointer = EXT_CZO

CODEFILE_PTH_COL_3 1  "${Q}/EXAMPLE/OBS/"
  ## widget = initmenu; pointer = DIR_PZH

CODEFILE_EXT_COL_3 1  "PZH"
  ## widget = initmenu; pointer = EXT_PZH

CODEFILE_PTH_COL_4 1  "${Q}/EXAMPLE/OBS/"
  ## widget = initmenu; pointer = DIR_PZO

CODEFILE_EXT_COL_4 1  "PZO"
  ## widget = initmenu; pointer = EXT_PZO

! A Priori Coordinates
! --------------------
COORD 1  "${Q}/EXAMPLE/STA/EDT2021430.CRD"
  ## widget = selwin; path = DIR_CRD; ext = EXT_CRD; maxfiles = 1
  # EDT2$YSS+0

DESCR_COORD 1  "A priori coordinates"

! Eccentricities
! --------------
ECCENT 0
  ## widget = selwin; path = DIR_ECC; ext = EXT_ECC; maxfiles = 1
  ## emptyallowed = true
  # 

DESCR_ECCENT 1  "Site eccentricities"

! Troposphere
! ---------
TROPEST 1  "${Q}/EXAMPLE/ATM/EDT2021430.TRP"
  ## widget = selwin; path = DIR_TRP; ext = EXT_TRP; maxfiles = 1
  ## emptyallowed = true
  # EDT2$YSS+0

DESCR_TROPEST 1  "Estimated troposphere values"

! LEO Kinematic positions
! -----------------------
LEOPROC 1  "0"
  ## widget = checkbox

MSG_LEOPROC 1  "LEO files"

! LEO Standard Orbit
! ------------------
LEOSTD 0
  ## widget = selwin; activeif = LEOPROC = 1; path = DIR_STD; ext = EXT_STD
  ## maxfiles = 1; emptyallowed = true
  # 

DESCR_LEOSTD 1  "LEO standard orbit"

! Kinematic Input Coordinates
! ---------------------------
KININP 0
  ## widget = selwin; path = DIR_KIN; ext = EXT_KIN; maxfiles = 1
  ## emptyallowed = true
  # 

DESCR_KININP 1  "Kin. input coordinates"

! LEO Attitude Data
! -----------------
ATTIT 0
  ## widget = selwin; activeif = LEOPROC = 1; path = DIR_ATT; ext = EXT_ATT
  ## maxfiles = 1; emptyallowed = true
  # 

DESCR_ATTIT 1  "LEO attitude"

! GPS-UTC file
! -------------
GPSUTC 1  "${X}/GEN/GPSUTC."
  ## widget = selwin; path = PTH_GEN; ext = NO_EXT; maxfiles = 1
  # GPSUTC.

DESCR_GPSUTC 1  "Difference GPS-UTC"

! Differentail Code Biases
! ------------------------
DCBINP 1  "${Q}/EXAMPLE/ORB/IGS021430.DCB"
  ## widget = selwin; path = DIR_DCB; ext = EXT_DCB; maxfiles = 1
  ## emptyallowed = true
  # $B$YSS+0

DESCR_DCBINP 1  "Code bias input files"

! Station Observation sigma factors for scaling the outlier limits
! ----------------------------------------------------------------
STAWGT 0
  ## widget = selwin; path = DIR_SOS; ext = EXT_SOS; maxfiles = 1
  ## emptyallowed = true
  # 

DESCR_STAWGT 1  "Station sigma factors"

! Resulting Coordinates
! ---------------------
COORDRS 0
  ## widget = lineedit; path = DIR_CRD; ext = EXT_CRD
  # 

DESCR_COORDRS 1  "Coordinate results"

! Resulting Kinematic Coordinates
! -------------------------------
KINOUT 0
  ## widget = lineedit; path = DIR_KIN; ext = EXT_KIN
  # 

DESCR_KINOUT 1  "Kinematic Coordinates"

! Residuals
! ---------
RESIDRS 0
  ## widget = lineedit; path = DIR_RES; ext = EXT_RES
  # 

DESCR_RESIDRS 1  "Residual file"

! Clock RINEX output file name
! -----------------------------
CLKRNXRS 0
  ## widget = lineedit; path = DIR_RXC; ext = EXT_RXC
  # 

DESCR_CLKRNXRS 1  "Clock RINEX results"

! Resulting Satellite Clocks
! --------------------------
SACLKRS 0
  ## widget = lineedit; path = DIR_CLK; ext = EXT_CLK
  # 

DESCR_SACLKRS 1  "Satellite clock results"

! GNSS receiver LC DCB values
! --------------------------
DCBOUT 0
  ## widget = lineedit; path = DIR_DCB; ext = EXT_DCB
  # 

DESCR_DCBOUT 1  "GNSS receiver LC DCB values"

! Summary Files
! -------------
SMCINO 1  "${Q}/EXAMPLE/OUT/VAL021430.SMC"
  ## widget = lineedit; path = DIR_SMC; ext = EXT_SMC
  # VAL$YSS+0

DESCR_SMCINO 1  "Output summary (XYZ coord.)"

SMEINO 0
  ## widget = lineedit; path = DIR_SME; ext = EXT_SME
  # 

DESCR_SMEINO 1  "Output summary (Ell. coord.)"

! Scratch Files
! -------------
AUXFIL 1  "${U}/WORK/CODSPP.SCR"
  ## widget = lineedit; path = PTH_SCR; ext = EXT_SCR; emptyallowed = false
  # CODSPP$J

DESCR_AUXFIL 1  "Scratch file 1"

AUXFIL1 1  "${U}/WORK/CODSPP.SC1"
  ## widget = lineedit; path = PTH_SCR; ext = EXT_SC1; emptyallowed = false
  # CODSPP$J

DESCR_AUXFIL1 1  "Scratch file 2"

AUXFIL2 1  "${U}/WORK/CODSPP.SC2"
  ## widget = lineedit; path = PTH_SCR; ext = EXT_SC2; emptyallowed = false
  # CODSPP$J

DESCR_AUXFIL2 1  "Scratch file 3"

DELETE_FILES 3
  "AUXFIL"
  "AUXFIL1"
  "AUXFIL2"

! Program Output File
! -------------------
SYSODEF 1  "0"
  ## widget = checkbox

MSG_SYSODEF 1  "Program output"

SYSOUT 1  "${Q}/EXAMPLE/OUT/VAL$(CLUSTER).OUT"
  ## widget = lineedit; path = DIR_OUT; ext = EXT_OUT
  ## activeif = SYSODEF == 0; emptyallowed = false
  # VAL$(CLUSTER)

DESCR_SYSOUT 1  "Program output"

! Error Message File
! ------------------
ERRMRG 1  "0"
  ## widget = checkbox

MSG_ERRMRG 1  "Error message"

SYSERR 1  "${U}/WORK/ERROR.MSG"
  ## widget = lineedit; path = PTH_ERR; ext = EXT_ERR
  ## activeif = ERRMRG == 0; emptyallowed = false
  # ERROR

DESCR_SYSERR 1  "Error message"

! Title
! -----
TITLE 1  "CLKDET_2002_$(CLUSTER)"
  ## widget = lineedit
  # CLKDET_$Y+0_$(CLUSTER)

MSG_TITLE 1  "Title line"

! Frequency
! ---------
FREQ 1  "L3"
  ## widget = combobox; editable = false; cards = L1 L2 L3

MSG_FREQ 1  "Frequency"

! Clock Polynomial Degree
! -----------------------
CLKPOLY 1  "1"
  ## widget = combobox; editable = false; cards = E 0 1 2 3 4 5 6 7

MSG_CLKPOLY 1  "Clock polynomial degree"

! Save Clock Estimates ?
! ----------------------
CLKSAVE 1  "NO"
  ## widget = combobox; editable = false; cards = NO CODE PHASE BOTH

MSG_CLKSAVE 1  "Save clock estimates"

! Estimate Coordinates ?
! ----------------------
COORDEST 1  "0"
  ## widget = combobox; editable = false; cards = NO STATIC KINEMATIC

MSG_COORDEST 1  "Estimate coordinates"

! Tropospheric Model
! ------------------
TROPOS 1  "NONE"
  ## widget = combobox; editable = false
  ## cards = NONE SAASTAMOINEN HOPFIELD MARINI-MUR ESTIMATED

MSG_TROPOS 1  "Troposphere"

! Ionosperic Model
! ----------------
IONOS 1  "0"
  ## widget = checkbox

MSG_IONOS 1  "Ionosphere"

! Minimal Elevation
! -----------------
MINEL 1  "20"
  ## widget = spinbox; range = 0 90 1

MSG_MINEL 1  "Minimum elevation"

! Sampling Rate
! -------------
SAMPLE 1  "1"
  ## widget = spinbox; range = 1 600 1

MSG_SAMPLE 1  "Sampling rate"

! Use mark flags from observation file
! ------------------------------------
USEMRK 1  "1"
  ## widget = checkbox

MSG_USEMRK 1  "Use mark flags from observation files"

! Use Obs. Window
! ---------------
WINDOW 1  "0"
  ## widget = checkbox

MSG_WINDOW 1  "Observation window"

! Observation Window
! ------------------
RADIO_1 1  "1"
  ## widget = radiobutton; group = DUMMY
  ## radiokeys = SESSION_YEAR SESSION_STRG

MSG_RADIO_1 1  "Defined by year and session number"

RADIO_2 1  "0"
  ## widget = radiobutton; group = DUMMY

MSG_RADIO_2 1  "Defined by start and end time"

SESSION_YEAR 1  "2002"
  ## widget = lineedit; multilineallowed = true; emptyallowed = false
  # $Y+0

MSG_SESSION_YEAR 1  "Year for sessions def. the time window"

SESSION_STRG 1  "1430"
  ## widget = lineedit; multilineallowed = true; emptyallowed = false
  # $S+0

MSG_SESSION_STRG 1  "Sessions defining the time window"

STADAT 1  "2002 05 23"
  ## widget = lineedit; activeif = RADIO_2 = 1; check_type = date
  # $YMD_STR+0

MSG_STADAT 1  "Start of time window (year month day)"

STATIM 1  "00 00 00"
  ## widget = lineedit; emptyallowed = false
  ## activeif = RADIO_2 = 1 AND STADAT / _; check_type = time

MSG_STATIM 1  "Start of time window (hour min. sec.)"

ENDDAT 1  "2002 05 23"
  ## widget = lineedit; activeif = RADIO_2 = 1; check_type = date
  # $YMD_STR+0

MSG_ENDDAT 1  "End of time window (year month day)"

ENDTIM 1  "23 59 59"
  ## widget = lineedit; emptyallowed = false
  ## activeif = RADIO_2 = 1 AND ENDDAT / _; check_type = time

MSG_ENDTIM 1  "End of time window (hour min. sec.)"

! Print Residuals
! ---------------
PRTRES 1  "0"
  ## widget = checkbox

MSG_PRTRES 1  "Residuals"

! Print Elevations
! ----------------
PRTELE 1  "0"
  ## widget = checkbox

MSG_PRTELE 1  "Elevations"

! Maximum Number of Iterations
! ----------------------------
ITRMAX 1  "10"
  ## widget = spinbox; range = 1 20 1

MSG_ITRMAX 1  "Max. number of iterations"

! Outlier Detection
! -----------------
OUTDET 1  "0"
  ## widget = checkbox

MSG_OUTDET 1  "Outlier detection"

! Maximum Residual Allowed
! ------------------------
RESMAX 1  "30.0"
  ## widget = lineedit; check_type = real; check_min = 0.0
  ## activeif = OUTDET = 1 AND COORDEST /= KINEMATIC

MSG_RESMAX 1  "Max. residual allowed"

! Confidence Interval
! -------------------
CONFIN 1  "5.0"
  ## widget = lineedit; check_type = real; check_min = 0.0
  ## activeif = OUTDET = 1 AND COORDEST /= KINEMATIC

MSG_CONFIN 1  "Confidence interval"

! Minimal Degree of Freedom
! -------------------------
KINDOF 1  "1"
  ## widget = spinbox; range = 0 5 1
  ## activeif = OUTDET = 1 AND COORDEST = KINEMATIC

MSG_KINDOF 1  "Min. degree of freedom"

! Maximum RMS of Epoch Solution
! -----------------------------
KINSIG 1  "5.0"
  ## widget = lineedit; check_type = real; check_min = 0.0
  ## activeif = OUTDET = 1 AND COORDEST = KINEMATIC

MSG_KINSIG 1  "Max. RMS of kin. solution"

! Mark outliers in obs. file ?
! ----------------------------
OUTLSAVE 1  "NO"
  ## widget = combobox; editable = false; cards = NO CODE PHASE BOTH
  ## activeif = OUTDET = 1

MSG_OUTLSAVE 1  "Mark outliers in obs. files"

! Header of the new RINEX file: RUNBY
! -----------------------------------
RUNBY 1  "AIUB"
  ## widget = lineedit

MSG_RUNBY 1  "Run by"

! Header of the new RINEX file: AC
! --------------------------------
AC 1  "CODE"
  ## widget = lineedit

MSG_AC 1  "AC"

! Header of the new RINEX file: ACName
! ------------------------------------
ACNAME 1  "Center for Orbit Determination of Europe"
  ## widget = lineedit

MSG_ACNAME 1  "AC name"

! Header of the new RINEX file: Comments
! ------------------------------------
COMMENT 2
  "STATION CLOCK INFORMATION"
  "BASED ON CODE POINT POSITIONING"
  ## widget = uniline

MSG_COMMENT 1  "Comment lines"


# BEGIN_PANEL NO_CONDITION #####################################################
# SINGLE POINT POSITIONING USING CODE MEASUREMENTS - CODSPP 1: Filenames       #
#                                                                              #
# GENERAL FILES                                                                #
#   Show all general files> % <                                                # SHOWGEN
#                                                                              #
# INPUT ORBITS                                                                 #
#   > % < Broadcast orbits> %%%%%%%% <                                         # RADIO_B BRDEPH
#   > % < Standard orbits > %%%%%%%% <       Satellite clocks      > %%%%%%%% <# RADIO_S STDORB SATCLK
# INPUT FILES                                                                  #
#   Code observation files> %%%%%%%% <       A priori coordinates  > %%%%%%%% <# CODEFILE COORD
#   Estimated tropo.values> %%%%%%%% <       Site eccentricities   > %%%%%%%% <# TROPEST ECCENT
#   Pole file             > %%%%%%%% <       Kin. input coordinates> %%%%%%%% <# POLE KININP
#   Station sigma factors > %%%%%%%% <       Code bias input files > %%%%%%%% <# STAWGT DCBINP
#   LEO files             > % <                                                # LEOPROC
# END_PANEL ####################################################################


# BEGIN_PANEL SHOWGEN = 1 ######################################################
# CODSPP 1.1: General Files                                                    #
#                                                                              #
# GENERAL INPUT FILES                                                          #
#   General constants           > %%%%%%%%%%%% <                               # CONST
#   Subdaily pole model         > %%%%%%%%%%%% <                               # SUBMOD
#   Nutation model              > %%%%%%%%%%%% <                               # NUTMOD
#   Satellite information       > %%%%%%%%%%%% <                               # SATELL
#   Receiver information        > %%%%%%%%%%%% <                               # RECEIVR
#   Satellite problems          > %%%%%%%%%%%% <                               # SATCRUX
#   Station information         > %%%%%%%%%%%% <                               # STAINFO
#   Geodetic datum              > %%%%%%%%%%%% <                               # DATUM
#   Phase center eccentricities > %%%%%%%%%%%% <                               # PHASECC
#                                                                              #
# MENU SETTINGS                                                                #
#   Selected campaign           > %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%% <# CAMPAIGN
#   Selected session              year> %%%% <  session> %%%% <                # YR4_INFO SES_INFO
#   Session table               > %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%% <# SESSION_TABLE
#                                                                              #
# TEMPORARY FILES                                                              #
#   Scratch files               > %%%%%%%% <   > %%%%%%%% <   > %%%%%%%% <     # AUXFIL AUXFIL1 AUXFIL2
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL LEOPROC = 1 ######################################################
# CODSPP 1.2: LEO Files                                                        #
#                                                                              #
# LEO FILES                                                                    #
#   LEO standard orbit    > %%%%%%%% <                                         # LEOSTD
#   LEO attitude          > %%%%%%%% <                                         # ATTIT
#   GPS-UTC file          > %%%%%%%% <     (only with JASON attitude file)     # GPSUTC
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# CODSPP 1.3: Output Files                                                     #
#                                                                              #
# RESULT FILES                                                                 #
#   Coordinate results          > %%%%%%%% <                                   # COORDRS
#   Kinematic coordinates       > %%%%%%%% <                                   # KINOUT
#   Residual file               > %%%%%%%% <                                   # RESIDRS
#   Satellite clock results     > %%%%%%%% <                                   # SACLKRS
#   Clock RINEX results         > %%%%%%%% <                                   # CLKRNXRS
#   GNSS receiver LC DCB values > %%%%%%%% <                                   # DCBOUT
#                                                                              #
# OUTPUT FILES                                                                 #
#   Output summary (XYZ coord.) > %%%%%%%% <                                   # SMCINO
#   Output Summary (Ell.coord.) > %%%%%%%% <                                   # SMEINO
#                                                                              #
# GENERAL OUTPUT FILES                                                         #
#   Program output              > % < use CODSPP.Lnn           or > %%%%%%%% < # SYSODEF SYSOUT
#   Error messages              > % < merged to program output or > %%%%%%%% < # ERRMRG SYSERR
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# CODSPP 2: Input Options                                                      #
#                                                                              #
# TITLE > %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%% <   # TITLE
#                                                                              #
# PARAMETERS                                                                   #
#   Frequency                             > %%%%%% <                           # FREQ
#   Clock polynomial degree               > %%%%%% <   E: one offset per epoch # CLKPOLY
#   Save clock estimates                  > %%%%%% <                           # CLKSAVE
#   Estimate coordinates                  > %%%%%%%%%%%%% <                    # COORDEST
#                                                                              #
# ATMOSPHERE MODELS                                                            #
#   Troposphere                           > %%%%%%%%%%%%% <                    # TROPOS
#   Ionosphere                            > % <                                # IONOS
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# CODSPP 3: Input Options                                                      #
#                                                                              #
# OBSERVATION SELECTION                                                        #
#   Minimum elevation                     > %% <  degrees                      # MINEL
#   Sampling rate                         > %% <                               # SAMPLE
#   Observation window                    > % <                                # WINDOW
#   Use mark flags from observation files > % <                                # USEMRK
#                                                                              #
# PRINT OPTIONS                                                                #
#   Residuals                             > % <                                # PRTRES
#   Elevations                            > % <                                # PRTELE
#                                                                              #
# END_PANEL ####################################################################	


# BEGIN_PANEL WINDOW = 1 #######################################################
# CODSPP 3.1: Observation Window                                               #
#                                                                              #
# OBSERVATION WINDOW                                                           #
#                                                                              #
#   > % < Defined by year and session number                                   # RADIO_1
#         Year  > %%%% <   Session > %%%% <                                    # SESSION_YEAR SESSION_STRG
#                                                                              #
#                                                                              #
#   > % < Defined by start and end time                                        # RADIO_2
#                 yyyy mm dd     hh mm ss           yyyy mm dd     hh mm ss    #
#         Start > %%%%%%%%%% < > %%%%%%%% <   End > %%%%%%%%%% < > %%%%%%%% <  # STADAT STATIM ENDDAT ENDTIM
#                                                                              #
# END_PANEL ####################################################################


# BEGIN_PANEL NO_CONDITION #####################################################
# CODSPP 4: Screening Options                                                  #
#                                                                              #
# ITERATIONS                                                                   #
#   Max. number of iterations   > %% <                                         # ITRMAX
#                                                                              #
# OUTLIER DETECTION                                                            #
#   Outlier detection           > % <                                          # OUTDET
#   Max. residual allowed       > %%%%% <  meters                              # RESMAX
#   Confidence interval         > %%%%% <  (in units of one sigma)             # CONFIN
#   Min. degree of freedom      > % <                                          # KINDOF
#   Max. RMS of kin. solution   > %%%%  <  meters                              # KINSIG
#   Mark outliers in obs. files > %%%%%% <                                     # OUTLSAVE
# END_PANEL ####################################################################	


# BEGIN_PANEL CLKRNXRS / _ #####################################################
# CODSPP 5: Header For Clock RINEX Files                                       #
#                                                                              #
# HEADER ENTRIES FOR THE CLOCK RINEX FILE                                      #
#   Run by   > %%%%%%%%%%%%%%%%%%% <                                           # RUNBY
#   AC       > %%% <                                                           # AC
#   AC name  > %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%% <        # ACNAME
#   Comment lines                                                              #
#      > %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%% <        # COMMENT
#                                                                              #
# END_PANEL ####################################################################
